[LONGITUDINAL]
input = {V, k, a}

EQUATION:
f = 100/V*exp(-k*t)

DEFINITION:
y = {distribution=lognormal, prediction=f, sd=a}

EQUATION: 
z=log(y)

DEFINITION:
u = {distribution=normal, prediction=z, sd=1}
